Procedure: Preliminary: Part 1 –in California, U.S.

1. To build the maze:
   * 1. Nail the two 6 inches, by 2 foot, by ¼ inch planks perpendicular, to the two 6 inch, by 4 foot, by ¼ inch planks.
     2. Nail the 4-foot by 2 foot perforated wooden wallboard to it, as it’s base.
     3. Mark the 3 thin wooden rods at 4 inch intervals
     4. Using the hand saw, cut the rods at these locations (creating 36, 4 inch rods)
     5. Place these smaller rods in the perforations at desired locations
     6. Using the blade cut strips out of the hard cardboard and place them between the rods, forming the pattern of the desired maze configuration.
     7. Finally, place the plastic sheet over the apparatus
2. Label the corridors of the maze, A through N and decide upon the orientation